BR2_arm=y
BR2_cortex_a9=y
BR2_ARM_ENABLE_NEON=y
BR2_ARM_ENABLE_VFP=y
BR2_ARM_FPU_VFPV3=y

# Linux headers same as kernel, a 4.11 series
BR2_PACKAGE_HOST_LINUX_HEADERS_CUSTOM_4_11=y

# System
BR2_TARGET_GENERIC_GETTY_PORT="ttymxc3"

# Bootloader
BR2_TARGET_UBOOT=y
BR2_TARGET_UBOOT_BUILD_SYSTEM_KCONFIG=y
BR2_TARGET_UBOOT_CUSTOM_VERSION=y
BR2_TARGET_UBOOT_CUSTOM_VERSION_VALUE="2017.07-rc1"
BR2_TARGET_UBOOT_BOARD_DEFCONFIG="imx6qdl_icore_mmc"
BR2_TARGET_UBOOT_NEEDS_DTC=y
BR2_TARGET_UBOOT_NEEDS_OPENSSL=y
BR2_TARGET_UBOOT_FORMAT_DTB_IMG=y
BR2_TARGET_UBOOT_SPL=y
BR2_TARGET_UBOOT_SPL_NAME="SPL"

# Kernel
BR2_LINUX_KERNEL=y
BR2_LINUX_KERNEL_CUSTOM_VERSION=y
BR2_LINUX_KERNEL_CUSTOM_VERSION_VALUE="4.11.5"
BR2_LINUX_KERNEL_DEFCONFIG="imx_v6_v7"
BR2_LINUX_KERNEL_UIMAGE=y
BR2_LINUX_KERNEL_UIMAGE_LOADADDR="0x10008000"
BR2_LINUX_KERNEL_DTS_SUPPORT=y
BR2_LINUX_KERNEL_INTREE_DTS_NAME="imx6dl-icore imx6q-icore"

# Filesystem
BR2_TARGET_GENERIC_ISSUE="Welcome to Engicam i.CoreM6 Quad/Dual/DualLite/Solo Starter Kit"
BR2_TARGET_ROOTFS_EXT2=y
BR2_TARGET_ROOTFS_EXT2_4=y
BR2_PACKAGE_HOST_DOSFSTOOLS=y
BR2_PACKAGE_HOST_GENIMAGE=y
BR2_PACKAGE_HOST_MTOOLS=y
BR2_ROOTFS_POST_IMAGE_SCRIPT="support/scripts/genimage.sh"
BR2_ROOTFS_POST_SCRIPT_ARGS="-c board/engicam/icorem6/genimage.cfg"
